SMS Alert based on combined forecast less than 4MW

API forecast based on coordinate as input to model

Machine learning Model based on historical data

Maintenance Schedule to calibrate the output from the ML predictions

Dashboard to display power availability when all constraints have been included

50 MW wind farm

10MW solar power plant